**SH120-II Digital microhematocrit centrifuge**



Spec:

|  |  |
| --- | --- |
| Brushless motor available, easy & safe-to-use, low noise, touch key interface. | |
| Max speed | 12000rpm Stepless regulation |
| Max rcf | 15300xg |
| Capactiy | dia 1.5mm\*75mm(24capillary tubes) |
| Timer | 0-99min |
| Digital display | Yes, speed indication, digital control panel |
| Power Supply | AC 220V/110V 50Hz/60Hz |
| Safety control | Mechanical lid lock. Auto pause device (Automatic stop when lid is open during operation) |

Packaging Details

Pack: carton (1 set in 1 box)   
G.W/N.W: 11kg/10kg   
Size: 28L\*31W\*27H (cm) 图片包含 图形用户界面

描述已自动生成

